
New spring cage for dummy functions


**The new spring cage is used with ALX and ND both the 170 & 172 dummy functions.**



**-Single cast part.**

**- will surface mount. (Through bolt is optional.)**

Old spring cage for dummy functions



**-Assembled machined parts. (Requires through bolt)**